#

##

##

    µVision Build Log
    Project:
    E:\Y\keil\ZDBMS\ZDBMS\MCUCore.uvproj
    Project File Date:  01/23/2025

    Output:
    Build target 'McuFlash_Load'
    compiling Main.c...
    compiling Initial.c...
    compiling InterruptApp.c...
    compiling Led.c...
    compiling KeyApp.c...
    compiling LowPower.c...
    compiling UartApp.c...
    compiling Memory.c...
    compiling AFE.c...
    compiling Balance.c...
    compiling Calculate.c...
    compiling Calibrate.c...
    compiling ChargerLoad.c...
    compiling ExtE2PRom.c...
    compiling Interrupt.c...
    compiling KeyScan.c...
    compiling McuFlash.c...
    compiling McuLib.c...
    CODE_DRV\MCULIB.C(20): warning C280: 'ClkSource': unreferenced local variable
    CODE_DRV\MCULIB.C(84): warning C280: 'SysClock': unreferenced local variable
    compiling MosCtrl.c...
    compiling PorSelfTest.c...
    compiling Protect.c...
    compiling RTC.c...
    compiling TWI.c...
    compiling Uart.c...
    compiling Thermistor.c...
    compiling TwiIO.c...
    assembling STARTUP.A51...
    compiling GasGaugeInter_V4_13.c...
    compiling BootApp.c...
    compiling BootIAP.c...
    linking...
    *** WARNING L15: MULTIPLE CALL TO SEGMENT
        SEGMENT: ?PR?_MCUCLOCKSET?MCULIB
        CALLER1: ?PR?INTERRUPTINT4?INTERRUPT
        CALLER2: ?C_C51STARTUP
    Program Size: data=151.4 xdata=1529 code=29770
    creating hex file from ".\output\MCUCore_Load"...
    ".\output\MCUCore_Load" - 0 Error(s), 3 Warning(s).
    Load "E:\\Y\\keil\\ZDBMS\\ZDBMS\\output\\MCUCore_Load"
    Flash Erase Done.
    ISP size=0, E2PROM size=1024;
    Main Size=64512Bytes; E2PROM Size=1024Bytes;
    The Code CheckSum is 32F7H
    Code Write Done: 29776 bytes programmed.
    Code Option Write Done.
    Code Verify Done: 29776 bytes verified.
    Code Option Verify Done
    Code Security Write Done.
    Code Security Verify Done
    Update EEprom Done
    elaspe time 3985 ms
    Build target 'McuFlash_Load'
    compiling Main.c...
    compiling Initial.c...
    compiling InterruptApp.c...
    compiling Led.c...
    compiling KeyApp.c...
    compiling LowPower.c...
    compiling UartApp.c...
    compiling Memory.c...
    compiling AFE.c...
    compiling Balance.c...
    compiling Calculate.c...
    compiling Calibrate.c...
    compiling ChargerLoad.c...
    compiling ExtE2PRom.c...
    compiling Interrupt.c...
    compiling KeyScan.c...
    compiling McuFlash.c...
    compiling McuLib.c...
    CODE_DRV\MCULIB.C(20): warning C280: 'ClkSource': unreferenced local variable
    CODE_DRV\MCULIB.C(84): warning C280: 'SysClock': unreferenced local variable
    compiling MosCtrl.c...
    compiling PorSelfTest.c...
    compiling Protect.c...
    compiling RTC.c...
    compiling TWI.c...
    compiling Uart.c...
    compiling Thermistor.c...
    compiling TwiIO.c...
    assembling STARTUP.A51...
    compiling GasGaugeInter_V4_13.c...
    compiling BootApp.c...
    compiling BootIAP.c...
    linking...
    *** WARNING L15: MULTIPLE CALL TO SEGMENT
        SEGMENT: ?PR?_MCUCLOCKSET?MCULIB
        CALLER1: ?PR?INTERRUPTINT4?INTERRUPT
        CALLER2: ?C_C51STARTUP
    Program Size: data=151.4 xdata=1529 code=29607
    creating hex file from ".\output\MCUCore_Load"...
    ".\output\MCUCore_Load" - 0 Error(s), 3 Warning(s).
    Load "E:\\Y\\keil\\ZDBMS\\ZDBMS\\output\\MCUCore_Load"
    Flash Erase Done.
    ISP size=0, E2PROM size=1024;
    Main Size=64512Bytes; E2PROM Size=1024Bytes;
    The Code CheckSum is E552H
    Code Write Done: 29613 bytes programmed.
    Code Option Write Done.
    Code Verify Done: 29613 bytes verified.
    Code Option Verify Done
    Code Security Write Done.
    Code Security Verify Done
    Update EEprom Done
    elaspe time 3969 ms
    Build target 'McuFlash_Load'
    compiling Main.c...
    compiling Initial.c...
    compiling InterruptApp.c...
    compiling Led.c...
    compiling KeyApp.c...
    compiling LowPower.c...
    compiling UartApp.c...
    compiling Memory.c...
    compiling AFE.c...
    compiling Balance.c...
    compiling Calculate.c...
    compiling Calibrate.c...
    compiling ChargerLoad.c...
    compiling ExtE2PRom.c...
    compiling Interrupt.c...
    compiling KeyScan.c...
    compiling McuFlash.c...
    compiling McuLib.c...
    CODE_DRV\MCULIB.C(20): warning C280: 'ClkSource': unreferenced local variable
    CODE_DRV\MCULIB.C(84): warning C280: 'SysClock': unreferenced local variable
    compiling MosCtrl.c...
    compiling PorSelfTest.c...
    compiling Protect.c...
    compiling RTC.c...
    compiling TWI.c...
    compiling Uart.c...
    compiling Thermistor.c...
    compiling TwiIO.c...
    assembling STARTUP.A51...
    compiling GasGaugeInter_V4_13.c...
    compiling BootApp.c...
    compiling BootIAP.c...
    linking...
    *** WARNING L15: MULTIPLE CALL TO SEGMENT
        SEGMENT: ?PR?_MCUCLOCKSET?MCULIB
        CALLER1: ?PR?INTERRUPTINT4?INTERRUPT
        CALLER2: ?C_C51STARTUP
    Program Size: data=151.4 xdata=1529 code=29770
    creating hex file from ".\output\MCUCore_Load"...
    ".\output\MCUCore_Load" - 0 Error(s), 3 Warning(s).
    Load "E:\\Y\\keil\\ZDBMS\\ZDBMS\\output\\MCUCore_Load"
    Flash Erase Done.
    ISP size=0, E2PROM size=1024;
    Main Size=64512Bytes; E2PROM Size=1024Bytes;
    The Code CheckSum is 3315H
    Code Write Done: 29776 bytes programmed.
    Code Option Write Done.
    Code Verify Done: 29776 bytes verified.
    Code Option Verify Done
    Code Security Write Done.
    Code Security Verify Done
    Update EEprom Done
    elaspe time 4000 ms